**PART-1**All done in the Services Tab of the DHCP Server

**PART-2  
*Step-1:***R1>en  
R1>conf t  
R1(config)#interface gigabitEthernet 0/0  
R1(config-if)#ip helper-address 192.168.60.253  
R1(config-if)#exit  
R1(config)#exit  
R1#exit

***Step-2:***Done in PC1’s IP Configuration mode from Desktop

**PART-3**

***Step-1:***   
Went to the Web Browser from Desktop of PC1 and typed the addresses cisco.com and publicsite.com. The results are shown below: